**Cooler Master Enforcer Mid Tower Cabinet**

  
Rs. 6930

**Key Features of Cooler Master Enforcer Mid Tower Cabinet**

* 2 Fans
* Mid Tower Cabinet
* 2 Front USB 3.0 Port/ 2 Front USB 2.0 Ports
* 8 Expansion Slots
* Suitable for microATX, ATX Motherboards
* Power Supply Placement at Bottom

**Specifications of Cooler Master Enforcer Mid Tower Cabinet**

|  |  |
| --- | --- |
| **GENERAL** | |
| Series: | Storm Enforcer |
| Part Number: | SGC-1000-KWN1 |
| Motherboard Supported: | microATX, ATX |
| Type: | Mid Tower |
| Material: | Steel, ABS Plastic, Mesh |

|  |  |
| --- | --- |
| **COOLING** | |
| Cooling Solution Support: | Supported, Fan |
| Coolers - Front: | 1, 200 mm Fan |
| Coolers - Rear: | 1, 120 mm Fan |
| Fan LED: | Red |
| Radiator Support: | Supported |

|  |  |
| --- | --- |
| **BAYS AND EXPANSION SLOTS** | |
| Cable Management: | Yes |
| Expansion Slots : | 8 |
| 3.5 inch Bays: | 6 (Internal), 1 (External) |
| 5.25 inch Bays: | 4 (External) |
| SSD Drive Bays: | 4 (2.5 inch SSD Bay) |

|  |  |
| --- | --- |
| **PORTS AND SLOTS** | |
| USB 3.0 Ports: | 2 (Front) |
| USB 2.0 Ports: | 2 (Front) |
| Audio Jacks: | Microphone Jack |
| Other Connectors: | 1 x Audio |

|  |  |
| --- | --- |
| **POWER** | |
| Power Supply Enclosure: | Bottom of Cabinet |

|  |  |
| --- | --- |
| **ADDITIONAL FEATURES** | |
|  | Front Fan Speed - 1000 RPM, Fan Noise Level - 19 dBA, Rear Fan Speed - 1200 RPM, Fan Noise Level - 17 dBA, Dust Filters on Bottom and Front Intakes, Reinforced Front Door, Removable and Rotatable HDD Cage, Support High-end Graphics Cards, Storm Guard Security System |

|  |  |
| --- | --- |
| **DIMENSIONS** | |
| Dimensions: | 229 x 484.5 x 523.5 mm |
| Maximum Cooling Unit Height Supported: | 175 mm |
| Maximum Graphics Card Size: | 390 inch |
| Weight: | 8.9 kg |

|  |  |
| --- | --- |
| **WARRANTY** | |
| Domestic Term: | 2 Year |
| Service Type: | Carry In |
| Covered in Warranty: | Manufacturing Defects, Dead on Arrival |
| Not Covered in Warranty: | Physical Damages, Mishandling, Burnt Cases |
| Warranty Type: | Repair |
| Warranty Summary: | Customer Contact 1800-221-988 in case of support issues |

**Cooler Master Elite 310 Cabinet (Silver)**

Rs. 1826

**Key Features of Cooler Master Elite 310 Cabinet (Silver)**

* 1 Fan
* Mid Tower Cabinet
* 2 USB 2.0 Ports
* 7 Expansion Slots
* Suitable for microATX, ATX Motherboards
* Power Supply Placement on Top

**Specifications of Cooler Master Elite 310 Cabinet (Silver)**

|  |  |
| --- | --- |
| **IN THE BOX** | |
| Sales Package: | Cabinet case, Respective screws for fixing the Motherboard and Cables |

|  |  |
| --- | --- |
| **GENERAL** | |
| Series: | Cooler Master Elite 310 |
| Part Number: | RC-310-SKN1-GP |
| Motherboard Supported: | microATX, ATX |
| Type: | Mid Tower |
| Material: | Steel, ABS Plastic, Bezel |

|  |  |
| --- | --- |
| **COOLING** | |
| Cooling Solution Support: | Supported, Fan |
| Coolers - Rear: | 1, 120 x 25 mm Fan |

|  |  |
| --- | --- |
| **BAYS AND EXPANSION SLOTS** | |
| Expansion Slots : | 7 |
| 3.5 inch Bays: | 6 (Internal), 1 (External) |
| 5.25 inch Bays: | 4 (External) |

|  |  |
| --- | --- |
| **PORTS AND SLOTS** | |
| Other USB Ports: | 2 x USB 2.0 |
| Audio Jacks: | Microphone Jack |
| Other Connectors: | 1 x Audio |

|  |  |
| --- | --- |
| **POWER** | |
| Power Supply Enclosure: | Standard ATX PS2 enclosure at Top of Cabinet |

|  |  |
| --- | --- |
| **ADDITIONAL FEATURES** | |
|  | Rear Fan Speed - 1200 RPM, Fan Noise Level - 17 dBA, Easily Accessible I/O Panel, Side Panel Security Lock Hole, Side Ventilation Holes |

|  |  |
| --- | --- |
| **DIMENSIONS** | |
| Dimensions: | 191 x 437 x 468 mm |
| Weight: | 5.8 kg |

|  |  |
| --- | --- |
| **WARRANTY** | |
| Domestic Term: | 2 Year |
| Service Type: | Carry In |
| Covered in Warranty: | Manufacturing Defects, Dead on Arrival |
| Not Covered in Warranty: | Physical Damages, Mishandling, Burnt Cases |
| Warranty Type: | Repair |